**H-232图示均衡器 EQUALIZER**

****

**产品特点:**

图示双31段恒定Q值均衡器，1/3倍频程

30mm长推杆，更加精细调节系统

全SMT表面贴装工艺

双7段光柱电平

前面板旁通开关

带反馈点检测并指示，检测灵敏度可调

高切及低切开关功能，切点频率可调

Dual 31-segment constant Q equalizer, 1/3 octave

30mm long putter, finer adjustment system

Full SMT surface mount process

Double 7-segment beam level

Front panel bypass switch

With feedback point detection and indication, the detection sensitivity is adjustable

High cut and low cut switch function, adjustable cut point frequency