**Badao8000娱乐音箱**

**特点：**

1.独特合成材料纸盆，有效提高了话筒的柔顺性和稳定性

2.高品质滤波元件和卓越的无源滤波技术。

3.恒指向高音90º×60º，可根据实际使用场所旋转。

4.完善的吊装结构和安装点位设计，底部带支撑插孔。

**适用于娱乐会所和DISCO，慢摇吧及豪华娱乐包房，演艺大厅、现场表演、酒吧，多功能厅、宴会厅**

**1. Unique synthetic material paper cone, which effectively improves the flexibility and stability of the microphone**

**2. High quality filter components and excellent passive filtering technology.**

**3. Constant pointing treble 90o × 60o, can be rotated according to the actual use.**

**4. Perfect lifting structure and installation point design, with support socket at the bottom.**

**Suitable for entertainment clubs and DISCO, slow rocking and luxury entertainment rooms, performing arts halls, live performances, bars, multi-purpose halls, banquet halls**

**Badao8000**

产品参数Parameters:

单元组成Driver：LF1x 15" HF1x 3"

标称阻抗 Nominal Impedance: 8Ω


额定功率 Power Handling: 600W

频率响应 Frequency Range (+/-3 dB):40Hz -18kHz

辐射角度 Dispersion(-6 dB): H x V 90°x 60°

灵敏度 Sensitivity: 99dB

最大声压级：Maximum Peak SPL: 131dB

连接插座Connection:2x Speakon NL4

音箱尺寸Product dimensions(WxDxH):430x460x680mm

净重N.W:42KG